**INITIALIZE DEFAULT ANGLE TO ZERO.**

**METAL SERVO 2**

**METAL SERVO 1**

LET THERE BE A DELAY OF 1 SECOND WHEN THE MALLET IS ROTATED ABOUT 18 DEGREES EACH TIME FOR HITTING THETONE BAR**.**

**5**

**TOY SERVO 2**

**TOY SERVO 1**

**TONE BARS**

**6**

**8**

**7**

**TONE BARS**

**4**

**3**

**2**

**1**

WHEN THE MALLET IS TURNED TO AROUND 54 DEGREES REDIRECT TO INITIAL (DEFAULT) POSTIION